AutoGen Definitions dummy;
class = {
  cp-id     = 'class_i2_c_i_o';
  cp-name   = 'I2CIO';
  cp-section = {
    sec-kind = 'public-func';
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1a32eb7832075ad6011d67874405a0d0a6';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'I2CIO';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '51';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Constructor method
    @discussion Class constructor constructor. 
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1a6f814653d903dc2ff6e8420eeb7954ae';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
int
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'begin';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'i2cAddr';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '63';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   Initializes the device.
    @discussion This method initializes the device allocating an I2C address.
    This method is the first method that should be call prior to calling any
    other method form this class. On initialization all pins are configured
    as INPUT on the device.
    @param      i2cAddr: I2C Address where the device is located.
    @result     1 if the device was initialized correctly, 0 otherwise
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1a53b94274eb6bb68564cf5243323db887';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'pinMode';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'pin';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'dir';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '73';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   Sets the mode of a particular pin.
    @discussion Sets the mode of a particular pin to INPUT, OUTPUT. digitalWrite
    has no effect on pins which are not declared as output.
    @param      pin: Pin from the I2C IO expander to be configured. Range 0..7
    @param      dir: Pin direction (INPUT, OUTPUT).
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1a0341888753bc54c4384f5593a870fb34';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'portMode';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'dir';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '83';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   Sets all the pins of the device in a particular direction.
    @discussion This method sets all the pins of the device in a particular
    direction. This method is useful to set all the pins of the device to be
    either inputs or outputs.
    @param      dir: Direction of all the pins of the device (INPUT, OUTPUT).
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1a7a3db7bfc15ede0ae9e8c8bd44290ef7';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'read';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '93';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   Reads all the pins of the device that are configured as INPUT.
    @discussion Reads from the device the status of the pins that are configured
    as INPUT. During initialization all pins are configured as INPUTs by default.
    Please refer to pinMode or portMode.
    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1ac26221011a8b49bcea9ef62712ea88a7';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'digitalRead';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'pin';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '106';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   Read a pin from the device.
    @discussion Reads a particular pin from the device. To read a particular
    pin it has to be configured as INPUT. During initialization all pins are
    configured as INPUTs by default. Please refer to pinMode or portMode.
    @param      pin: Pin from the port to read its status. Range (0..7)
    @result     Returns the pin status (HIGH, LOW) if the pin is configured
    as an output, reading its value will always return LOW regardless of its
    real state.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1ae2063569c927d0008e2593d14504fdcd';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
int
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'write';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '120';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   Write a value to the device.
    @discussion Writes to a set of pins in the device. The value is the binary
    representation of all the pins in device. The value written is masked with 
    the configuration of the direction of the pins; to change the state of
    a particular pin with this method, such pin has to be configured as OUTPUT 
    using the portMode or pinMode methods. If no pins have been configured as
    OUTPUTs this method will have no effect.
    @param      value: value to be written to the device.
    @result     1 on success, 0 otherwise
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_i2_c_i_o_1a473206162522b847546777d16a7c6dcd';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
int
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'digitalWrite';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'pin';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'level';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '132';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   Writes a digital level to a particular pin.
    @discussion Write a level to the indicated pin of the device. For this 
    method to have effect, the pin has to be configured as OUTPUT using the
    pinMode or portMode methods.
    @param      pin: device pin to change level. Range (0..7).
    @para       level: logic level to set the pin at (HIGH, LOW).
    @result     1 on success, 0 otherwise.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-section = {
    sec-kind = 'private-attrib';
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_i2_c_i_o_1abcd6f7f5f176f965d8ae535afa9f6cec';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_shadow';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '137';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_i2_c_i_o_1a283a99ef1c6f58fa8a0489089cba9682';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_dirMask';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '138';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_i2_c_i_o_1ade58da873af4240a53053ef5f12a2728';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_i2cAddr';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '139';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_i2_c_i_o_1a8c566f3fd332eefe4db57cbe6b69337c';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
bool
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_initialised';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      sec-mem-desc-line = '140';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-filename  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
  cp-fileline  = '44';
  cp-briefdesc = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  cp-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* class */
class = {
  cp-id     = 'class_l_c_d';
  cp-name   = 'LCD';
  cp-ref     = {
    ref-type = derived;
    ref-id   = 'class_liquid_crystal';
    ref-prot = public;
    ref-virt = non-virtual;
  };
  cp-ref     = {
    ref-type = derived;
    ref-id   = 'class_liquid_crystal___i2_c';
    ref-prot = public;
    ref-virt = non-virtual;
  };
  cp-section = {
    sec-kind = 'public-func';
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a00bb2db1390721abc7b24ac4b8c276c8';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'LCD';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '104';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method
    @abstract   LiquidCrystal abstract constructor.
    @discussion LiquidCrystal class abstract constructor needed to create
    the base abstract class.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a5b7aee49867828a0160a142b9109c07a';
      sec-mem-virt = pure-virtual;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
virtual void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'begin';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'cols';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rows';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'charsize';
        sec-mem-param-defval = <<_EnD_oF_dEf_TeXt_
LCD_5x8DOTS
_EnD_oF_dEf_TeXt_;
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '120';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   LCD initialization.
    @discussion Initializes the LCD to a given size (col, row). This methods
    initializes the LCD, therefore, it MUST be called prior to using any other
    method from this class.

    This method is pure abstract, it is dependent on each derived class from
    this base class to implement the internals of how the LCD is initialized
    and configured.

    @param      cols the number of columns that the display has
    @param      rows the number of rows that the display has
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1afa699e0beeeee03cce8cef87eba81c4a';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'clear';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '132';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Clears the LCD.
    @discussion Clears the LCD screen and positions the cursor in the upper-left 
    corner. 

    This operation is time consuming for the LCD.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1aee45ad37f09312f5d9982257e2d37e68';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'home';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '145';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Sets the cursor to the upper-left corner.
    @discussion Positions the cursor in the upper-left of the LCD. 
    That is, use that location in outputting subsequent text to the display. 
    To also clear the display, use the clear() function instead.

    This operation is time consuming for the LCD.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1af3974da6d988ba2d21c25135ada12108';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'noDisplay';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '155';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Turns off the LCD display.
    @discussion Turns off the LCD display, without losing the text currently 
    being displayed on it.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a5b07cf05e8e5e7c53654f5ca0cf58b89';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'display';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '166';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Turns on the LCD display.
    @discussion Turns on the LCD display, after it's been turned off with 
    noDisplay(). This will restore the text (and cursor location) that was on 
    the display prior to calling noDisplay().

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a3b755c4b397b5985752be8c30ee1a9b5';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'noBlink';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '174';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Turns off the blinking of the LCD cursor.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a878b36878fa8287093964eba83aace77';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'blink';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '184';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Display the cursor of the LCD.
    @discussion Display the blinking LCD cursor. If used in combination with 
    the cursor() function, the result will depend on the particular display.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1aec8ffaa1e69c7a6e13ac0cfbc29151d9';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'noCursor';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '192';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Hides the LCD cursor.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a194814f64dfa50a90e07e0fe0d361620';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'cursor';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '202';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Display the LCD cursor.
    @discussion Display the LCD cursor: an underscore (line) at the location 
    where the next character will be written.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a6f3a503055b3b8dcf0f61b2633c584f7';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'scrollDisplayLeft';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '211';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Scrolls the contents of the display (text and cursor) one space 
    to the left.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1abfc44b294772f09020bfa32af8a79571';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'scrollDisplayRight';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '220';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Scrolls the contents of the display (text and cursor) one space 
    to the right.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a238e9f6476dc7df64af04eb6c87f6ac7';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'leftToRight';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '233';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Set the direction for text written to the LCD to left-to-right.
    @discussion Set the direction for text written to the LCD to left-to-right. 
    All subsequent characters written to the display will go from left to right, 
    but does not affect previously-output text.

    This is the default configuration.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1ac014830eadc26bfd86308ea8734f4428';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'rightToLeft';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '246';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Set the direction for text written to the LCD to right-to-left.
    @discussion Set the direction for text written to the LCD to right-to-left. 
    All subsequent characters written to the display will go from right to left, 
    but does not affect previously-output text.

    left-to-right is the default configuration.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1abb3ed88d530f6283e6159b4973e7da9e';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'autoscroll';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '261';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Turns on automatic scrolling of the LCD.
    @discussion Turns on automatic scrolling of the LCD. This causes each 
    character output to the display to push previous characters over by one 
    space. If the current text direction is left-to-right (the default), 
    the display scrolls to the left; if the current direction is right-to-left, 
    the display scrolls to the right. 
    This has the effect of outputting each new character to the same location on 
    the LCD.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a96035dde40efbf73390e00b5beb00231';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'noAutoscroll';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '271';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Turns off automatic scrolling of the LCD.
    @discussion Turns off automatic scrolling of the LCD, this is the default
    configuration of the LCD.

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a91cba8f93c692abcddf8bc3de58d2d3a';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'createChar';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'location';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'charmap';
        sec-mem-param-array = '[]';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '289';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Creates a custom character for use on the LCD.
    @discussion Create a custom character (glyph) for use on the LCD. 
    Most chipsets only support up to eight characters of 5x8 pixels. Therefore,
    this methods has been limited to locations (numbered 0 to 7). 

    The appearance of each custom character is specified by an array of eight 
    bytes, one for each row. The five least significant bits of each byte 
    determine the pixels in that row. To display a custom character on screen, 
    write()/print() its number, i.e. lcd.print (char(x)); // Where x is 0..7.

    @param      location: LCD memory location of the character to create
    (0 to 7)
    @param      charmap: the bitmap array representing each row of the character.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a48220450fd152b25994eb7d0ba340e8d';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'setCursor';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'col';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'row';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '300';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Position the LCD cursor.
    @discussion Sets the position of the LCD cursor. Set the location at which 
    subsequent text written to the LCD will be displayed.

    @param      col LCD column
    @param      row LCD row - line.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a31a0cb42497d83cdc9cb8000828f7190';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'command';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '314';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Send a command to the LCD.
    @discussion This method sends a command to the LCD by setting the Register
    select line of the LCD.

    This command shouldn't be used to drive the LCD, only to implement any other
    feature that is not available on this library.

    @param      value Command value to send to the LCD.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1acf471f0d9fea7ea3f5c3279519c8b32c';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
size_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'write';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '327';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Writes to the LCD.
    @discussion This method writes character to the LCD in the current cursor
    position.

    This is the virtual write method, implemented in the Print class, therefore
    all Print class methods will end up calling this method.

    @param      value Value to write to the LCD.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_l_c_d_1a121fac7d916284d71af8b1fdd9ade2f6';
      sec-mem-virt = pure-virtual;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
virtual void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'send';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'mode';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '342';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Send a particular value to the LCD.
    @discussion Sends a particular value to the LCD. This is a pure abstract
    method, therefore, it is implementation dependent of each derived class how
    to physically write to the LCD.

    Users should never call this method.

    @param      value Value to send to the LCD.
    @result     mode LOW - write to the LCD CGRAM, HIGH - write a command to
    the LCD.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-section = {
    sec-kind = 'protected-attrib';
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_l_c_d_1aef093ba3f8e1016267b40ac235a0fa0f';
      sec-mem-virt = normal;
      sec-mem-prot = protected;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_displayfunction';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '349';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_l_c_d_1ae47a0e2eff74431a39774b788d5761f4';
      sec-mem-virt = normal;
      sec-mem-prot = protected;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_displaycontrol';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '351';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_l_c_d_1a726b9a68d091dd8683a18e83f3a8fd3c';
      sec-mem-virt = normal;
      sec-mem-prot = protected;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_displaymode';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '353';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_l_c_d_1ac1374911fb145fea430c21092ada0c06';
      sec-mem-virt = normal;
      sec-mem-prot = protected;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_numlines';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      sec-mem-desc-line = '354';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-filename  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
  cp-fileline  = '95';
  cp-briefdesc = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  cp-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  cp-inheritancegraph = <<_EnD_oF_dEf_TeXt_
      node = {
        node-id    = 2;
        node-label = 'LCD';
        node-link = {
          node-link-id = 'class_l_c_d';
        };
      }; /* node */
      node = {
        node-id    = 3;
        node-label = 'LiquidCrystal';
        node-link = {
          node-link-id = 'class_liquid_crystal';
        };
        node-child = {
          child-id = '2';
          relation = public-inheritance;
        }; /* node-child */
      }; /* node */
      node = {
        node-id    = 4;
        node-label = 'LiquidCrystal_I2C';
        node-link = {
          node-link-id = 'class_liquid_crystal___i2_c';
        };
        node-child = {
          child-id = '2';
          relation = public-inheritance;
        }; /* node-child */
      }; /* node */

_EnD_oF_dEf_TeXt_;
}; /* class */
class = {
  cp-id     = 'class_liquid_crystal';
  cp-name   = 'LiquidCrystal';
  cp-ref     = {
    ref-type = base;
    ref-id   = 'class_l_c_d';
    ref-prot = public;
    ref-virt = non-virtual;
  };
  cp-section = {
    sec-kind = 'public-func';
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1a49d2bd8d26031a1c83bcbd73978a1686';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'LiquidCrystal';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rs';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'enable';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd0';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd1';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd2';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd3';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd4';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd5';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd6';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd7';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '50';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   8 bit LCD constructors.
    @discussion Defines the pin assignment that the LCD will have.
    The constructor does not initialize the LCD.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1a30e3d865c4b4a003a36cb45903f93644';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'LiquidCrystal';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rs';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rw';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'enable';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd0';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd1';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd2';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd3';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd4';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd5';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd6';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd7';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '53';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1a0a0a8dfa7a2e775a031fd65f5c6366ec';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'LiquidCrystal';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rs';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rw';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'enable';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd0';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd1';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd2';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd3';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '62';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   4 bit LCD constructors.
    @discussion Defines the pin assignment that the LCD will have.
    The constructor does not initialize the LCD.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1a23124e6dd5ac4a9b6147629b96e91953';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'LiquidCrystal';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rs';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'enable';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd0';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd1';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd2';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd3';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '64';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1adb5f37d69809ed7c0772c74a4adff19b';
      sec-mem-virt = virtual;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
virtual void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'begin';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'cols';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rows';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'charsize';
        sec-mem-param-defval = <<_EnD_oF_dEf_TeXt_
LCD_5x8DOTS
_EnD_oF_dEf_TeXt_;
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '79';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   LCD initialization.
    @discussion Initializes the LCD to a given size (col, row). This methods
    initializes the LCD, therefore, it MUST be called prior to using any other
    method from this class.

    @param      cols: the number of columns that the display has
    @param      rows: the number of rows that the display has
    @param      charsize: size of the characters of the LCD: LCD_5x8DOTS or
    LCD_5x10DOTS.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1a56142f8b3753bedd133e4139e5eb5089';
      sec-mem-virt = virtual;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
virtual void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'send';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'mode';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '93';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Send a particular value to the LCD.
    @discussion Sends a particular value to the LCD for writing to the LCD or
    as an LCD command.

    Users should never call this method.

    @param      value Value to send to the LCD.
    @result     mode LOW - write to the LCD CGRAM, HIGH - write a command to
    the LCD.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-section = {
    sec-kind = 'private-func';
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1ae45eec827b26174f73e9cf3ddda635af';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'init';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'fourbitmode';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rs';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rw';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'enable';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd0';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd1';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd2';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd3';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd4';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd5';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd6';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'd7';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '105';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Initializes the LCD pin allocation
    @discussion Initializes the LCD pin allocation and configuration.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1adebd21f2955b1e193a6d24367833fd63';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'write8bits';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '112';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Writes an 8 bit value to the LCD.
    @discussion Writes 8 bits to the LCD control data lines.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1a52837217db49272eea03c9056cab36a8';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'write4bits';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '119';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Writes an 4 bit value to the LCD.
    @discussion Writes 4 bits (the least significant) to the LCD control data lines.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal_1a44d84c010396c993f124d2feb9dc794d';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'pulseEnable';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '127';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Pulse the LCD enable line (En).
    @discussion Sends a pulse of 1 uS to the Enable pin to execute an command
    or write operation.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-section = {
    sec-kind = 'private-attrib';
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal_1affd20665bda00d8b0e37d5ee87543e81';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_rs_pin';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '129';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal_1a29061eaa64c2e9f3b985ff52249b62a9';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_rw_pin';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '130';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal_1aef7d920abae32b5faa2625ffa3879c4b';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_enable_pin';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '131';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal_1a0b2da39d056aed9940b0525e554668d7';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_data_pins';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
      sec-mem-desc-line = '132';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-filename  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
  cp-fileline  = '40';
  cp-briefdesc = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  cp-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  cp-inheritancegraph = <<_EnD_oF_dEf_TeXt_
      node = {
        node-id    = 7;
        node-label = 'LCD';
        node-link = {
          node-link-id = 'class_l_c_d';
        };
      }; /* node */
      node = {
        node-id    = 6;
        node-label = 'LiquidCrystal';
        node-link = {
          node-link-id = 'class_liquid_crystal';
        };
        node-child = {
          child-id = '7';
          relation = public-inheritance;
        }; /* node-child */
      }; /* node */

_EnD_oF_dEf_TeXt_;
  cp-collaborationgraph = <<_EnD_oF_dEf_TeXt_
      node = {
        node-id    = 9;
        node-label = 'LCD';
        node-link = {
          node-link-id = 'class_l_c_d';
        };
      }; /* node */
      node = {
        node-id    = 8;
        node-label = 'LiquidCrystal';
        node-link = {
          node-link-id = 'class_liquid_crystal';
        };
        node-child = {
          child-id = '9';
          relation = public-inheritance;
        }; /* node-child */
      }; /* node */

_EnD_oF_dEf_TeXt_;
}; /* class */
class = {
  cp-id     = 'class_liquid_crystal___i2_c';
  cp-name   = 'LiquidCrystal_I2C';
  cp-ref     = {
    ref-type = base;
    ref-id   = 'class_l_c_d';
    ref-prot = public;
    ref-virt = non-virtual;
  };
  cp-section = {
    sec-kind = 'public-func';
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1aac537d195557e0b8afac1a71441a484c';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'LiquidCrystal_I2C';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'lcd_Addr';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '84';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Class constructor. 
    @discussion Initializes class variables and defines the I2C address of the
    LCD. The constructor does not initialize the LCD.

    @param      lcd_Addr: I2C address of the IO expansion module. For I2CLCDextraIO,
    the address can be configured using the on board jumpers.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1aeee2ada537f0cfbfda8613324b57c4a6';
      sec-mem-virt = virtual;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
virtual void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'begin';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'cols';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'rows';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'charsize';
        sec-mem-param-defval = <<_EnD_oF_dEf_TeXt_
LCD_5x8DOTS
_EnD_oF_dEf_TeXt_;
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '98';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   LCD initialization.
    @discussion Initializes the LCD to a given size (col, row). This methods
    initializes the LCD, therefore, it MUST be called prior to using any other
    method from this class.

    @param      cols: the number of columns that the display has
    @param      rows: the number of rows that the display has
    @param      charsize: size of the characters of the LCD: LCD_5x8DOTS or
    LCD_5x10DOTS.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1a8bf1fab7efe13e8b17b96c42d1f810b4';
      sec-mem-virt = virtual;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
virtual void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'send';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-declname = 'mode';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '112';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Send a particular value to the LCD.
    @discussion Sends a particular value to the LCD for writing to the LCD or
    as an LCD command.

    Users should never call this method.

    @param      value: Value to send to the LCD.
    @result     mode: LOW - write to the LCD CGRAM, HIGH - write a command to
    the LCD.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1a576f1f5813f55f34333d6d7e9fe53ad3';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'noBacklight';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '122';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Switch-off the LCD backlight.
    @discussion Switch-off the LCD backlight, this method is not supported by
    the I2CLCDextraIO, it needs an extra IO pin to drive the LCD backlight

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1a9f296e0d26f8b6a4509d8d4b9d738c03';
      sec-mem-virt = normal;
      sec-mem-prot = public;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'backlight';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '132';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @function
    @abstract   Switch-on the LCD backlight.
    @discussion Switch-on the LCD backlight, this method is not supported by
    the I2CLCDextraIO, it needs an extra IO pin to drive the LCD backlight

    @param      none
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-section = {
    sec-kind = 'private-func';
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1a459c4fa106fb7bac5940e3c6aea736af';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
int
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'init';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '142';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Initializes the LCD class
    @discussion Initializes the LCD class and IO expansion module.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1aebb0b9f000b94cc3ab026e0154d6ecef';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'write4bits';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-defname = 'value';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '149';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Writes an 4 bit value to the LCD.
    @discussion Writes 4 bits (the least significant) to the LCD control data lines.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1a1d715dbf40f06b4c15004cd356b5a321';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'pulseEnable';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-defname = '_data';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '157';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Pulse the LCD enable line (En).
    @discussion Sends a pulse of 1 uS to the Enable pin to execute an command
    or write operation.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'function';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1a4c63780ceef67e90750d3e4bbdb83402';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
void
_EnD_oF_dEf_TeXt_;
      sec-mem-name = 'expanderWrite';
      sec-mem-param = {
        sec-mem-param-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
        sec-mem-param-defname = '_data';
      }; /*        sec-mem-param--param */
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '165';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_
    @method     
    @abstract   Writes to the expansion module.
    @discussion Writes a byte to the IO expansion module. This will be applied
    to all its outputs.
_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-section = {
    sec-kind = 'private-attrib';
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1a0bb3cc7ec414b373ef00e0cc6642ec88';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_Addr';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '167';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1af99934fdb39403e02d68981ad8366e6b';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_cols';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '168';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1adb3edf6c68b018a37293a926c4816127';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_rows';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '169';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1af63a2b732d345d55abfcb83bf962c8d3';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
uint8_t
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_backlightval';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '170';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
    sec-member = {
      sec-mem-kind = 'variable';
      sec-mem-id   = 'class_liquid_crystal___i2_c_1adcc89f14c444ff086f544f33fc18ca4c';
      sec-mem-virt = normal;
      sec-mem-prot = private;
      sec-mem-type = <<_EnD_oF_dEf_TeXt_
I2CIO
_EnD_oF_dEf_TeXt_;
      sec-mem-name = '_i2cio';
      sec-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      sec-mem-desc-line = '171';
      sec-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      sec-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* sec-member */
  }; /* cp-section */
  cp-filename  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
  cp-fileline  = '72';
  cp-briefdesc = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  cp-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  cp-inheritancegraph = <<_EnD_oF_dEf_TeXt_
      node = {
        node-id    = 11;
        node-label = 'LCD';
        node-link = {
          node-link-id = 'class_l_c_d';
        };
      }; /* node */
      node = {
        node-id    = 10;
        node-label = 'LiquidCrystal_I2C';
        node-link = {
          node-link-id = 'class_liquid_crystal___i2_c';
        };
        node-child = {
          child-id = '11';
          relation = public-inheritance;
        }; /* node-child */
      }; /* node */

_EnD_oF_dEf_TeXt_;
  cp-collaborationgraph = <<_EnD_oF_dEf_TeXt_
      node = {
        node-id    = 13;
        node-label = 'LCD';
        node-link = {
          node-link-id = 'class_l_c_d';
        };
      }; /* node */
      node = {
        node-id    = 12;
        node-label = 'LiquidCrystal_I2C';
        node-link = {
          node-link-id = 'class_liquid_crystal___i2_c';
        };
        node-child = {
          child-id = '13';
          relation = public-inheritance;
        }; /* node-child */
        node-child = {
          child-id = '14';
          relation = usage;
          edgelabel = <<_EnD_oF_dEf_TeXt_
_i2cio
_EnD_oF_dEf_TeXt_;
        }; /* node-child */
      }; /* node */
      node = {
        node-id    = 14;
        node-label = 'I2CIO';
        node-link = {
          node-link-id = 'class_i2_c_i_o';
        };
      }; /* node */

_EnD_oF_dEf_TeXt_;
}; /* class */
file = {
  file-id   = '_i2_c_i_o_8cpp';
  file-name = 'I2CIO.cpp';
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.cpp';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
file = {
  file-id   = '_i2_c_i_o_8h';
  file-name = 'I2CIO.h';
    define = {
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_i2_c_i_o_8h_1a218dbde2f6fda8c5825e25da10864c71';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = '_I2CIO_VERSION';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
"1.0.0"
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
      define-mem-desc-line = '34';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    };
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/I2CIO.h';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
file = {
  file-id   = '_l_c_d_8cpp';
  file-name = 'LCD.cpp';
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.cpp';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
file = {
  file-id   = '_l_c_d_8h';
  file-name = 'LCD.h';
    define = {
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1acc3509bc0442b41e2b816555de473ed2';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_CLEARDISPLAY';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x01
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '53';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_
 @defined 
 @abstract   All these definitions shouldn't be used unless you are writing 
 a driver.
 @discussion All these definitions are for driver implementation only and
 shouldn't be used by applications.
_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a154c86a887633d0f6d9988e4dbb1f419';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_RETURNHOME';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x02
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '54';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a5597e1d5819ea2f0734ad4313abf6703';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_ENTRYMODESET';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x04
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '55';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1adfb8b2b8b8a08d7313504d7a4f89d99f';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_DISPLAYCONTROL';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x08
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '56';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a61f16a2b7550e4700f7898a7587c5594';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_CURSORSHIFT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x10
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '57';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1aaef882ae70d1f485cd132815d9716111';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_FUNCTIONSET';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x20
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '58';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1aae6ea856879c11dee58493184582a52f';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_SETCGRAMADDR';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x40
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '59';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a15008b832807a208d9d88c74e6751ebf';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_SETDDRAMADDR';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x80
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '60';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a43c26ba2e66880fac95ef640b56873ad';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_ENTRYRIGHT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '64';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1ae7c6309fce6200bd7526d090a4a84dd0';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_ENTRYLEFT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x02
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '65';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1aa2cf1d0f4a319e53c009cffe1184466c';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_ENTRYSHIFTINCREMENT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x01
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '66';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a049ee97e98d04788c1da9a55590fbe42';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_ENTRYSHIFTDECREMENT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '67';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a76236ae8317b34bbc98ea56bc0a2639c';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_DISPLAYON';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x04
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '71';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a257ebe775cac7140cf82aa40d8ce545a';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_DISPLAYOFF';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '72';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1ab67f0adccde68de88eee0513fdfc4574';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_CURSORON';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x02
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '73';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a32b194a3adaa0a0bb69acee2e6a754fa';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_CURSOROFF';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '74';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1ac3b19d4e6553b9bbf18a23387e439206';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_BLINKON';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x01
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '75';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a4b28243034cec656b0ed490ba6979752';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_BLINKOFF';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '76';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1ab2f7b67abfac33f610acfd5d7a971f40';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_DISPLAYMOVE';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x08
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '80';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1ac21f0302ac4136775877d5f4759e4f74';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_CURSORMOVE';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '81';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1acf5999180233790bb2c9902efde58f7f';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_MOVERIGHT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x04
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '82';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1aafb86adb0dfca1e65d65b2cd1946a009';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_MOVELEFT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '83';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a59a57ca857dae5d89eb5f2a38c4ac6f0';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_8BITMODE';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x10
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '87';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1ab8c35d355d2372090c7a347e961c9224';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_4BITMODE';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '88';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a7987e93538df2819583ba43b81ddbb25';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_2LINE';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x08
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '89';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a8c85cf88d8af66a47c42249d81c94641';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_1LINE';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '90';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1abb3210156d88d3fe18c9352eb161fe42';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_5x10DOTS';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x04
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '91';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_l_c_d_8h_1a9ef57e724c1b846dae0f531aff6fb464';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_5x8DOTS';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
      define-mem-desc-line = '92';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    };
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LCD.h';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
file = {
  file-id   = '_liquid_crystal_8cpp';
  file-name = 'LiquidCrystal.cpp';
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.cpp';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
file = {
  file-id   = '_liquid_crystal_8h';
  file-name = 'LiquidCrystal.h';
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal.h';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
file = {
  file-id   = '_liquid_crystal___i2_c_8cpp';
  file-name = 'LiquidCrystal_I2C.cpp';
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.cpp';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
file = {
  file-id   = '_liquid_crystal___i2_c_8h';
  file-name = 'LiquidCrystal_I2C.h';
    define = {
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_liquid_crystal___i2_c_8h_1ac059d24dfe9c1e1f7c07cb7869a1833b';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_BACKLIGHT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x00
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      define-mem-desc-line = '41';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_liquid_crystal___i2_c_8h_1a65fa786d6e31fe8b1aa51784a9736581';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'LCD_NOBACKLIGHT';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
0x80
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      define-mem-desc-line = '42';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_liquid_crystal___i2_c_8h_1ab5ef25ebfe582f7bf0d93e2770548e2c';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'En';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
B01000000
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      define-mem-desc-line = '54';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_
 @warning These definitions will have to be changed should the IOExpander be 
 connected differently to this default.


 @defined 
 @abstract   Enable bit of the LCD
 @discussion Defines the IO of the expander connected to the LCD Enable
_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_liquid_crystal___i2_c_8h_1a98b6a2661a04ebbc1b3f38da70306814';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'Rw';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
B00100000
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      define-mem-desc-line = '61';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_
 @defined 
 @abstract   Read/Write bit of the LCD
 @discussion Defines the IO of the expander connected to the LCD Rw pin
_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    define-member = {
      define-mem-kind = 'define';
      define-mem-id   = '_liquid_crystal___i2_c_8h_1a345d1a871beb9e772c3bf9ef75412bb5';
      define-mem-virt = normal;
      define-mem-prot = public;
      define-mem-name = 'Rs';
      define-mem-initializer = <<_EnD_oF_dEf_TeXt_
B00010000
_EnD_oF_dEf_TeXt_;
      define-mem-desc-file = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
      define-mem-desc-line = '68';
      define-mem-briefdesc =    <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
      define-mem-documentation = <<_EnD_oF_dEf_TeXt_
 @defined 
 @abstract   Register bit of the LCD
 @discussion Defines the IO of the expander connected to the LCD Register select pin
_EnD_oF_dEf_TeXt_;
    }; /* define-member */
    };
  file-full-name  = '/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.h';
  file-first-line = '1';
  file-briefdesc  = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
  file-documentation = <<_EnD_oF_dEf_TeXt_

_EnD_oF_dEf_TeXt_;
}; /* file */
